25.09.2026 KHAN YACHT COMPLETED WORKS LIST
Rigging Operations
1. All rigging was inspected; wires, ropes, pulleys, turnbuckles, and Norseman terminals deemed necessary were replaced.
2. The genoa sail tack fitting chrome was replaced. Sail washing and renewal maintenance were performed.
3. A chrome davit/bracket was made for the accommodation ladder.
4. The mizzen mast boom was raised, and the position of the sheet pad eye was changed.
Painting and Varnishing Works 5. Scaffolding was erected up to the bulwarks, and the entire vessel, including the top, was covered. The paint color was changed with a new paint job, and the bulwarks were varnished. Antifouling paint was applied. 6. All varnished areas on the yacht were completely scraped and sanded; impregnating filler varnish was applied, colored, and finished with topcoat polyurethane varnishes. 7. The bilge was cleaned and painted with Danboline paint.
Electrical Works 8. All pumps on the yacht were checked and maintained. The entire electrical system, solar energy panels, inverter, battery chargers, and batteries were checked. 9. A new boiler (water heater) was purchased and installed. 10. The air conditioning system was checked and maintained.
Carpentry Works 11. Rot on the topsides and underwater hull was repaired. 12. Deck seams were leveled, and new Burmese teak strips were tightly glued. All cracks on the cabin sides were opened and repaired with new wood. 13. Cracked teak on the deck was replaced, and tight caulking/repairs were made. 14. Port and starboard bow and stern coverings, the forecastle, rubbing strakes, and rotten areas on the cockpit seating were opened and repaired with epoxy and new solid wood. 15. The seating group in the inner cockpit was removed, and rotten areas were repaired. The upholstery was renewed. A new bar with a custom-made refrigerator was built. The instrument panel in the wheelhouse was replaced, and a visor was made for it. 16. Portholes and saloon windows were removed and tightened to ensure watertightness, necessary gaskets were replaced, and they were reinstalled. 17. Rot caused by water ingress on the cabin sides and under the saloon seating group was cleaned and repaired. 18. The passerelle grating was removed, replaced with a new one made of Burmese teak, and firmly repaired. 19. Rot on the engine beds, floors, and stern tube area was cleaned and repaired. 20. The crew cabin hatch glass was replaced; the bases and frames of the other hatches were repaired. 21. Rot on the crew cabin bathroom floor was cleaned, fiberglassed, and tiled with ceramics; a new toilet was purchased and installed.
Mechanical Works 22. Main engines and generators were maintained; the shaft and propeller were removed, crack-tested, and reinstalled. Stern tube cutlass bearings were replaced. 23. Plumbing systems were checked, hoses were replaced with odorless sanitation hoses, and black/grey water tanks were cleaned. 24. The toilet and fixtures in the captain's cabin bathroom were replaced.
Documentation / Paperwork 25. Tourism operation license, Radio license, Tonnage certificate, Ship health certificate, and Seaworthiness certificate were obtained.
Equipment Completion / Outfitting 26. New kitchen preparation tools, utensils, and presentation equipment were purchased and completed. 27. Dining table chairs were purchased. 28. New textile products for accommodation (bedspreads, pillowcases, bed sheets, towels, etc.) were purchased and completed. The yacht's logo was embroidered on the required textile products.
Sincerely,

